VESSELS NAME - OMSKIY-109

IMO - 8875621

TYPE - SINGLEDECKER

FLAG - RUSSIAN

BUILT - 1982

CLASS - RMRS KM \* Л4 R2 RSN

PANDI CLUB - SOGAZ.

GT/NT - 2463 / 979

SUMMER DWT - 3174MTS

SUMMER DWCC - ABT 3040MTS

DRAFT (SSW) - 3.26 M

GEARED - N/A GEARLESS

LOA/BEAM - 108.4 М/14,8М

GRAIN IN MAIN HOLD - 4383 CBM GRAIN

HOLDS/HATCHES - 4/4

HATCH SIZES -

15.8\*11.2 M

15.8\*11.2 M

15.8\*11.2 M

15.8\*11.2 M

TYPE OF HATCHCOVERS (WHICH TO BE IN GOOD WORKING CONDITION) - MCGREGOR

HORSE POWER - 2\*515 KWT

SERVICE SPEED - ACCORDING TO SHIP’S DOCUMENTS

MAX PRESSURE ON HOLDS BOTTOM - 5,0 MTS/PSQM, ON HATCHES - 1,7 MTS/PSQM

THE AVERAGE SPEED 8.2 KNOTS SUBJECT SEA 2 BEAUFORT

DAILY CONSUMPTION AT SEA (AVERAGE SPEED 8,2 KN, SEA - 2 BEAUFORT): DIESEL OIL (MGO) - 3,7 MT.

DAILY CONSUMPTION IN PORT: DIESEL OIL (MGO) - 0,3 MT

ALL ABOVE MENTIONED IS ABOUT (+/- 5%)

BUNKER-----ISO 8217 2010, MGO SULFUR NOT EXCEED 0,1%