VESSEL’S NAME - VTS-2

IMO - 8422644

TYPE - GENERAL CARGO

FLAG - RUSSIA

BUILT - 1984

CLASS - КМ \* L4 R2 –RSN

PANDI CLUB - VSK

GT/NT - 1572/585 MT

SUMMER DWT - 2162 T.

SUMMER DWCC – 2053,4T.

DRAFT (SWT) - 3.90 M

GEARED - N/A GEARLESS

LOA/BEAM - 82.45 M /11.60 M

GRAIN IN MAIN HOLD - 1820 M3

HOLDS/HATCHES - 2/2

HATCH SIZES №1 - 21.9X9.2 M

HATCH SIZES №2 - 21.4X9.2 M

TYPE OF HATCH COVERS (WHICH TOBE IN GOOD WORKING CONDITION):

HYDRAULICS

HORSE POWER - 2X441 KWT

SERVICE SPEED - ACCORDING TO SHIP’S DOCUMENTS

MAX PRESSURE ON HOLDS BOTTOM – 7.0 MTS/ AN HATCHES – 1.55 MTS

THE AVERAGE SPEED 7.5 KNOTS SUBJECT SEA 2 BEAU FORT

DAILY CONSUMPTION AT SEA (AVERAGE SPEED 7.5 KNOTS SUBJECT SEA 2 BEAU FORT):

DIESEL OIL(MGO) – 3.4 MT

DAILY CONSUMPTION IN PORT: DIESEL OIL (MGO) - 0.432 MT

ALL ABOVE MENTIONED IS ABOUT (=/- 5%)

BUNKER ---- IOS. MGO SULFUR NOT EXCEED 0.1%